**Computer Memory**

**Computer Memory**: Refers to the storage space within a computer where data and instructions are stored for processing.

* **CPU Access**: Computer memory allows the CPU to quickly retrieve information, which is essential for efficient processing.
* **Bit**: The smallest unit of memory is called a **bit**, which stands for **binary digit**. It can hold a value of either 0 or 1.
* **Flip-Flop**: The location where a single bit (0 or 1) is stored is called a **flip-flop**.
* **Storage Capacity**: A flip-flop can store **one bit of data**.
* **Register**: A collection of two or more flip-flops is called a **register**. Registers are used to hold data temporarily for quick access by the CPU.
* **Fastest Memory Units**: Registers and Cache Memory are the fastest types of memory.
* **Expensive Computer Memory**: The most expensive types of computer memory are **Registers**, **Cache Memory**, and **RAM**.
* **Slowest Memory**: The slowest type of computer memory is the **Disk** (such as Hard Disk Drives or HDDs and Solid-State Drives or SSDs).

**Data Access Hierarchy in Computer Architecture**

**CPU Searches Data in Registers**:

* The CPU first looks for the needed data in its **registers**.

**CPU Searches Data in Cache**:

* If the data is not found in the registers, the CPU then checks the **cache memory**.

**Cache Searches Data in Main Memory**:

* If the data is not in the cache, the CPU retrieves it from **main memory (RAM)**.

**Main Memory Searches Data in Secondary Memory**:

* If the data is not found in main memory, it will then be fetched from **secondary memory** (like a hard disk or SSD).

**Registers and Cache Memory: Key Components in CPU Data Access**

**Registers:**

* Registers are **not part of the main memory**.
* They are the **smallest and fastest** type of memory in a computer.
* located directly on the CPU chip
* They hold small amounts of data that the CPU needs immediately.
* Registers is a **temporary storage**.
* **Registers** hold a small amount of data, usually ranging from **32 bits** to **64 bits**.

**Cache Memory**:

* **Cache Memory** are **part of the main memory**.
* They are the **smallest (1st register) and fastest (1st register)** type of memory in a computer.
* located close to the CPU
* Cache memory is typically **volatile**, meaning it loses its contents when the power is turned off.
* **Acts as a Buffer Between RAM and the CPU** => **Cache memory** acts like a waiting area between the CPU and RAM. It keeps often-used data and instructions close by so the CPU can access them quickly, making the computer run faster and work more efficiently.
* **Cache Hit**: If the required data is found in the cache, it is quickly retrieved, leading to faster processing.
* **Cache Miss**: If the required data is not found in the cache, the CPU must fetch it from the slower main memory, which takes more time.

**TYPES OF CACHE MEMORY**

* Level 1 / Register (L1)
* Level 2 / Cache Memory (L2)
* Level 3 / Main Memory (L3)
* Level 4 / Secondary Memory (L4)

A white background with black text and black text

Description automatically generated**Memory Units:**

* **1 Bit** = Binary Digit
* **4 Bits** = 1 Nibble
* **8 Bits** = 1 Byte
* **1024 Bytes** = 1 KB (Kilobyte)
* **1024 KB** = 1 MB (Megabyte)
* **1024 MB** = 1 GB (Gigabyte)
* A white board with black text and black text

  Description automatically generated**1024 GB** = 1 TB (Terabyte)
* **1024 TB** = 1 PB (Petabyte)
* **1024 PB** = 1 EB (Exabyte)
* **1024 EB** = 1 ZB (Zettabyte)
* **1024 ZB** = 1 YB (Yottabyte)
* **1024 YB** = 1 BB (Brontobyte)
* **1024 BB** = 1 Geop Byte

A white sign with black text

Description automatically generatedA white sign with black text and yellow text

Description automatically generated

**The Role of Data and Instructions in Computer Operations**

**Data** refers to the information that the computer processes and manipulates. This can include:

* **Numbers:** Integers, floating-point numbers, etc.
* **Text:** Characters, strings, and text files.
* **Images:** Bitmap or vector graphics.
* **Audio and Video:** Media files such as MP3, WAV, MP4, etc.
* **Variables:** Values that can change during program execution.

**Example:** In a database application, data could be the records of customers, including names, addresses, and phone numbers.

**Instructions** are commands that tell the computer what operations to perform on the data. They are part of a program. The instructions **guide** the CPU on what tasks to perform. The CPU **follows** these instructions step by step to complete the program. This can include:

* **Arithmetic Operations:** Add, subtract, multiply, divide.
* **Control Flow:** Conditional statements (if-else), loops (for, while).
* **Input/Output Operations:** Reading data from or writing data to devices.
* **Data Manipulation:** Sorting, searching, or modifying data.

**Example:** In a simple program, an instruction might be to calculate the sum of two numbers and store the result in a variable.

A diagram of a computer memory

Description automatically generated

A diagram of a computer

Description automatically generated

**Primary Memory**

**Primary memory**, also known as **"main memory"** or **"internal memory,".**

**Characteristics of Primary Memory:**

* **Location:** It is located on the **motherboard** of the computer.
* **Connection:** It is **directly connected to the CPU,** which allows for fast data access and processing.
* **Purpose:** It temporarily **stores data and instructions** that the CPU is currently using or will need shortly.
* **Volatility:** It is often volatile, meaning the data is lost when the computer is turned off (in the case of RAM).

**RAM VS ROM**

A screenshot of a computer program

Description automatically generated

**SRAM VS DRAM**

A screenshot of a computer

Description automatically generated

**SDRAM**

A screenshot of a computer

Description automatically generated

**ROM TYPES**

* **PROM (Programmable Read-Only Memory)**
* **EPROM** (Erasable Programmable Read-Only Memory)
* **EEPROM** (Electrically Erasable Programmable Read-Only Memory)

**PROM (Programmable Read-Only Memory)**

* **Characteristics**: A type of ROM that can be programmed once after it's made.
* **When to use it**: Ideal for applications where the data won’t need to change, like certain firmware in devices.
* **How it works**: Data is written by burning out tiny connections in the chip, which means it can’t be changed later.

**2. EPROM (Erasable Programmable Read-Only Memory)**

* **Characteristics**: A type of ROM that can be erased and reprogrammed multiple times.
* **When to use it**: Useful when you might want to update the data, such as in firmware updates.
* **How it works**: You can erase the data by exposing the chip to ultraviolet (UV) light, and then reprogram it.

**3. EEPROM (Electrically Erasable Programmable Read-Only Memory)**

* **Characteristics**: A more flexible version of EPROM that can be erased and rewritten electrically.
* **When to use it**: Common in devices like computers for things that need to be updated often, like BIOS settings.
* **How it works**: You can erase and rewrite the data electronically, and it can be done one byte at a time.

**Storage Devices (Secondary Memory)**

**A screenshot of a video

Description automatically generated**

**Secondary memory**, also known as **secondary storage** or **auxiliary memory**, refers to a computer's long-term storage for programs and data. Unlike primary memory (like RAM), which is volatile and loses its contents when the power is off, secondary memory retains data even when the computer is turned off.

**Characteristics of Secondary Memory**

**Persistent Storage**:

* This means that the data stays saved even when the computer is turned off. You don’t lose your files unless you decide to delete them or overwrite them with new information.

**Capacity**:

* Secondary memory usually has a much larger storage capacity than primary memory (like RAM). This allows you to store a lot more data, such as documents, photos, videos, and applications.

**Speed**:

* Accessing data from secondary memory is generally slower than accessing data from primary memory. However, advancements in technology, like Solid State Drives (SSDs), are making secondary memory faster than it used to be.

**Cost**:

* Secondary memory is usually more affordable for storing large amounts of data compared to primary memory. This makes it a cost-effective option for users who need to store a lot of information.

**Examples of secondary memory devices**

**Optical Disc**

* CD (Compact Disc)
* DVD (Digital Versatile Disc)
* Blu-ray Disc
* MiniDisc
* LaserDisc
* Ultra HD Blu-ray

**Magnetic Disk**

* Hard Disk Drive (HDD)
* Floppy Disk
* Zip Disk
* Jazz Disk
* SuperDisk

**Magnetic Tape**

* Cassette Tape
* VHS Tape
* DAT (Digital Audio Tape)
* LTO (Linear Tape-Open)
* Reel-to-Reel Tape
* Magnetic Stripe Tape

**Solid-State Storage (also known as flash storage)**

* Pen Drives (USB Flash Drives)
* SD Cards
* Micro-SD Cards
* SIM Card (Although mainly for telecommunications, it does contain flash memory for data storage)
* Solid-State Disks (SSD)
* Flash Memory

**Understanding Disk vs. Disc: Types of Storage Media Explained**

* **Disk:** Refers to magnetic storage devices.
* **Disc:** Refers to optical storage devices.

**Methods for Data Accessing in Secondary Memory**

When it comes to accessing data stored in secondary memory, there are primarily two methods:

* **Sequential Access** and **Random Access**.

**Sequential Access**

**A diagram of a function

Description automatically generated**

**Definition**: Sequential access is a method of accessing data in a linear order, one item after another.

**How It Works**: When you want to find something, the system starts at the beginning of the data and goes through it line by line or record by record. It keeps checking each piece of data until it finds what you’re looking for.

**Example**: Imagine you have a long list of names. If you want to find a specific name, you would start at the top of the list and read each name until you reach the one you want.

Only **Magnetic Tape list include in** Sequential access.

**Examples:**

* **Tape Drives:** Tapes store data sequentially, requiring physical movement to access different parts of the tape.
* **Text Files:** Reading a text file line by line involves sequential access.
* **Audio and Video Files:** Playing audio or video files sequentially requires accessing the data in a linear order.

**Random Access**

**A diagram of a number

Description automatically generated**

**Definition:** Random access is a method of accessing data in a storage where any data item can be accessed directly without having to search in order.

**How It Works**: Random access lets the system quickly find and get data from any part of its storage. It uses special codes called addresses that tell it exactly where the data is located. This way, the system doesn’t have to look through everything one by one. Instead, it can go straight to the spot where the information is. Because of this, you don’t have to wait to find what you’re looking for. Overall, random access makes it much faster and easier to access data.

**Example**: It’s like having a digital library where you can go straight to the book you want without walking through the entire library.

**Optical Disk and Magnetic Disk** are example of Random Access

**Examples:**

* **Hard Drives:** Think of a hard drive like a library with many bookshelves. To find a specific book, you need to move the bookshelf to the correct position. The "seek mechanism" in a hard drive is like this, moving the reading head to the right part of the disk to find your data.
* **Solid-State Drives (SSDs):** Imagine an SSD as a digital filing cabinet. Each file is stored in a specific drawer. You can open any drawer directly without having to search through others. This is how SSDs work; they can access any data quickly without moving parts.
* **Random Access Memory (RAM):** Think of RAM as a really fast desk where you keep your most important papers. You can grab any paper you need instantly because it's right there. RAM is like this for your computer; it stores data that needs to be accessed quickly.

**RANDOM ACCESS VS SEQUENTIAL ACCESS**

|  |  |  |
| --- | --- | --- |
| **Parameter** | **Random Access** | **Sequential Access** |
| Definition | Allows data to be accessed in any order, directly from any location on the storage device. | Requires data to be accessed in a specific sequence. |
| How It Works | You can get to any data right away, no matter where it is. | You have to go through the data in order, one step at a time. |
| Speed | It's faster when you need specific data quickly. | It's slower because you have to go through everything step by step. |
| Best For | Good for tasks where you need data often and at random times. | Good for tasks where you go through data in a set order. |
| Where It's Used | Used in computers and phones where quick access is important. | Used in computers and phones where quick access is important. |
| Examples | Examples include computer memory (RAM), hard drives, and SSDs. | Examples include things like tape backups and some disk files. |

**Magnetic Tape**

Magnetic tape is a storage device made of a long, skinny strip of plastic that has a special coating on it. This coating can be changed by magnets, allowing it to hold data. It has been an important tool for saving and recording data for many years.

**Key characteristics of magnetic Tape:**

**1. Sequential access**: You can only read data in the order it’s stored. If you want to find something specific, you may have to fast-forward or rewind to get to it.

**2.High storage capacity:** Magnetic tape can store large amounts of data, so it can be used for backup purposes.

**3.Durability**: When stored correctly, magnetic tape can last for many years

**4.Cost-effective**: Magnetic tape is usually cheaper than other storage options, making it a budget-friendly option.

**Common uses of magnetic Tape:**

**Magnetic tapes** are used for large computers like mainframe.

**Audio and video recording**: Cassette tapes and VHS tapes are popular examples of magnetic tape used for recording music and movies.

**Data storage**: Magnetic tape is used to store data, especially for backups and long-term storage.

**Types of magnetic tape:**

**Reel-to-reel**: This is the old-fashioned that comes on large spools of tape

**Cartridge**: This type is in small cases, like music cassettes which makes them easy to use and transport.

**Data tape**: These tapes are made specifically for storing data and are often used in data centers.

Magnetic disk

Magnetic disk is a storage device used to store data. It has a round disk made of a non-magnetic material, which is covered with a magnetic layer. Data is stored in the form of magnetic fields on the surface of the platter.

A wire on a circular object

Description automatically generated

**Key characteristics of magnetic disk:**

**Random access**: Allows data to be accessed directly from any location on the storage device.

**High storage capacity:** Magnetic disk can store large amounts of data, so it can be used for backup purposes.

**Durability**: If stored correctly, magnetic disk can last for many years,

**Cost-effective**: Magnetic disk is usually cheaper than other storage options, making it a budget-friendly option.

**Features**

**Connected to**: Hard disks connect to the **motherboard**, which is the main circuit board in a computer.

**Data Cable**: Hard disks use different types of cables to connect and transfer data, including **PATA** (Parallel ATA), **SCSI** (Small Computer System Interface), and **SATA** (Serial ATA). SATA is the most common type used today.

**Speed Measured in**: The speed of a hard disk is measured in **RPM (Revolutions Per Minute)**,

**Speed**: Most hard disks typically have speeds ranging from **5400 RPM to 7200 RPM**.

**First Hard Disk**: Introduced in **1956** by **IBM**.

**Founder**: **Reynold B. Johnson**

**PATA Cable**:

* Stands for **Parallel Advanced Technology Attachment**.
* **Maximum Speed**: **133 MB/s**.

**SATA Cable**:

* Stands for **Serial Advanced Technology Attachment**.
* **Maximum Speed**: Ranges from **150 MB/s** to **600 MB/s** (with SATA III).

**SCSI**:

* Stands for **Small Computer System Interface**.
* **Maximum Speed**: Up to **640 MB/s** (varies by SCSI type).

When data is written to a hard disk, it is stored in the **sectors**.

**Smallest Physical Storage Unit**: Sector

**Sector Size**: **512 Bytes** (0.5 kB)

**Maximum Hard Disk Size**: **20 TB** (terabytes)

**Common Hard Disk Sizes**:

* **2.5-inch** (often used in laptops)
* **3.5-inch** (commonly used in desktop computers)

**Seek Time**:

* This is the time how long it takes for the hard disk’s read/write head to move to the right place on the disk to find the data you want. Think of it like finding a book on a shelf; it’s how long it takes to get to the right section.

**Latency Time**:

* This is the delay you experience after you ask for data until you actually get it. It’s like waiting for a specific page in a book to be right in front of you. This includes the time it takes for the disk to spin around so that the requested data is under the read/write head.

**Floppy Disks:**

**Also called as**: Floppy or diskette

**Developed**: It was developed by **IBM** in 1971

**Invented by**: **Alan Shugart**

**Data Written:** In a series of sectors

**Size**: Floppy disks come in different sizes: **3.5 inches**, **5.25 inches**, and **8 inches**.

* **3.5-inch disk**: Can hold **1.44 MB** of data (this is the most common size).
* **5.25-inch disk**: Can hold **up to 1.2 MB** of data for double-sided disks; **160 KB** for single-sided disks.
* **8-inch disk**: Can hold up to **minimum 80 KB and maximum 1.2 MB** of data.

 The 8-inch floppy disk was eventually replaced by smaller floppy disks, such as the 5.25-inch and 3.5-inch floppy disks, which had higher storage capacities.

**Flash Memory**

* Flash memory is an = **EEPROM** (Electrically Erasable Programmable Read-Only Memory). It allows data to be written, erased, and rewritten.
* It does not require a power source for working.
* Founder = Toshiba Company = Fujio Masuoka
* Pen Drive, SSD, and SD Card are valid examples of flash memory.
* NOR and NAND are types of flash memory

**SSD (Solid State Drive)**

**Definition**: An SSD (Solid State Drive) is a type of storage device that uses flash memory to store data.

**How It Works:** Traditional hard drives (HDDs) have spinning disks inside them, An SSD doesn’t have any moving parts; it uses memory chips instead, like what you find in a smartphone or a USB stick.

**Why is it better?**

**Speed:** SSDs are **way faster** than the old spinning hard drives. With an SSD, your computer starts up in seconds, apps open quickly, and files load almost instantly.

**Durable:** Since SSDs don’t have moving parts, they’re **less likely to break** if you accidentally drop

**Energy Efficiency:** SSDs use **less power** compared to traditional hard drives, which is great for laptops because it helps extend battery life.

**Size:**

* **2.5-inch SSD:** **used the SATA interface**
* **M.2 SSD:** for M.2 slot
* **PCIe SSD:** for special slot

**Downsides?**

* **More Expensive:** SSDs cost more than old hard drives

SSHD (Solid-State Hybrid Drive)

**Definition**: An SSHD is a **mix of an SSD and an HDD**. It has some memory chips like an SSD and a spinning disk like an HDD. This design aims to give you the **speed benefits of an SSD** while providing the **large storage capacity of an HDD**.

**How It Works:** The SSHD uses a small amount of **flash memory (like SSD storage)** to store data that you use the most. The rest of the data goes on the **spinning disk (like an HDD)**.

**Pros and Cons of SSHD**

**Pros:**

* Better Speed Than an HDD
* Larger Capacity Than an SSD
* **Cost-effective**

**Cons:**

* Slower than SSD
* More Complex than a Regular HDD or SSD

USB Device

A **USB (Universal Serial Bus) device** is a portable storage device or peripheral devices that connects to a computer or other device via a **USB port**. USB devices include flash drives, external hard drives, keyboards, mice, and other accessories.

**How It Works:** USB devices connect to a computer via **USB port**, and allows data transfer. USB storage devices use **flash memory** to store data, much like an SSD but in a smaller. USB devices help you **store data, transfer files, or control your computer**.

**Why is it better?**

**Portable:** USB devices are **small and lightweight**, so you can **easily carry them around**.

**Plug-and-Play:** Just plug them into the USB port, and the computer will usually recognize them without needing any extra software.

**Widely Compatible:** used in l**aptops, gaming consoles, smart TVs**

**Cost-effective**

**Speed**

**Types of USB Devices:**

* USB Flash Drives
* External Hard Drives/SSD
* **Peripherals (Keyboards, Mice, etc.):**
* USB Hubs

**Size and Versions:**

* **USB 2.0:**
* **USB 3.0/3.1:**
* USB-C

Downsides?

* Limited Lifespan
* Data Loss Risk:
* Speed Variability:

**Processor Components: ALU, CU, and Registers**

**CPU (Central Processing Unit)**

* **Also Known As**: Processor
* **Type**: Electronic circuit
* **Function**: Processes input data and produces output.
* The CPU does not have permanent memory; instead, it has temporary memory **=> Register**
* Primarily uses **serial processing** where GPU uses parallel processing

**Components**

1. **Control Unit (CU)**:
   * Responsible for decoding instructions.
   * Takes input **=>** Converts input into control signals **=>** Sends control signals to CPU
2. **Arithmetic Logic Unit (ALU)**:
   * Performs arithmetic and logical operations.
   * Building block of the CPU
3. **Memory Unit/Registers (MU)**:
   * CPU store data and instruction in MU
   * Temporary Memory

CPU Architecture

1. **RISC (Reduced Instruction Set Computer)**
2. CISC (Complex Instruction Set Computer)

**RISC**: Simpler, faster execution, fewer instructions.

**CISC**: More complex, greater flexibility, more instructions.

**CPU - 4 Basic Functions**

Fetch => Get the instruction from memory.

Decode => Understand what the instruction means and what needs to be done.

Execute => Perform the action specified by the instruction (like calculations).

Store => Save the results of the action back in memory or registers.

**Microprocessor**

* Latest form of processor or CPU.
* Small than processor (3rd generation)
* Part of the 4th generation of computers.
* **First Microprocessor**:
  + **Model**: Intel 4004
  + **Year Released**: 1971
* **Invented By**: Engineers at Intel.

**GPU (Graphics Processing Unit)**

* **What It Is**: A special type of processor for handling graphics and visual tasks.
* **Where It’s Used**: Commonly found in mobile phones to improve graphics performance.
* **Main Purpose**:
  + Helps with **video rendering** and making visuals look better.
* **How It Works**:
  + Uses **parallel processing**, which means it can do many tasks at the same time.
* **Popular Use**: Mainly used for **gaming** and other graphics-heavy applications.
* **Integration**: In mobile phones, the GPU is built into the main processor for better efficiency.

**Core Types in Processors**

**Dual-Core**: Processor with **2 cores**.

**Quad-Core**: Processor with **4 cores**.

**Hexa-Core**: Processor with **6 cores**.

**Octo-Core**: Processor with **8 cores**.