**Q) In the RISC architecture, what is meant by over lapping register window? Explain the relationship among register windows with over lapping register windows.**

**Overlapping register windows** are a feature found in some Reduced Instruction Set Computer (RISC) architectures. They provide a mechanism for efficient function calling and returning. This mechanism is especially useful in programming languages like C and Pascal, which frequently use function calls.

**How Overlapping Register Windows Work:**

1. Multiple Register Windows
2. Overlap
3. Window Pointer
4. Function Calls
5. Function Returns

**Multiple Register Windows:** The register file is divided into multiple register windows, each containing a set of registers.

**Overlap:** Adjacent register windows share some portion of their register. This means they have overlapping regions. This overlapping region (shared register) are used to pass arguments to functions and to return values.

**Window Pointer:** A special register called the "window pointer" keeps track of which register window is currently in use. This pointer is used for navigating between the overlapping register windows.

**Function Calls:** When a function is called:

* The window pointer is incremented to point to the next window.
* Arguments are passed into the overlapping region of the new window.
* The function's code executes in the new window.

**Function Returns:** When a function return:

* The window pointer is decremented to point to the previous window.
* The return value is placed in the overlapping region of the previous window.

**Benefits of Overlapping Register Windows:**

1. **Efficient Function Calls**
2. Reduced Memory Access
3. Simplified Compiler Implementation

**Efficient Function Calls:** By using the overlapping region, functions can directly access and share data without needing to save and restore it from registers, because data are kept in overlapping region, improving performance.

**Reduced Memory Access:** By keeping frequently used data in registers, memory accesses are reduced.

**Simplified Compiler Implementation:** The compiler can optimize function calls by placing arguments and return values in the overlapping region. This avoids data to save in register and restore from register. So, compilers can generate more optimized code, leading to faster execution.

**Relationship Among Register Windows:**

1. Sequential Register Windows
2. Circular Register Windows
3. SharingRegister Windows

**Sequential Register Windows**

Imagine a stack of plates. Each plate represents a register window. When you add a new plate to the stack, it overlaps with the top plate. This is similar to how sequential register windows work.

* **Each window** overlaps with its predecessor and successor.
* **When a function is called**, the window pointer moves to the next window, which overlaps with the current window. This overlap allows data to be passed between the two windows efficiently.
* **When a function returns**, the window pointer moves back to the previous window, again benefiting from the overlap.

**Circular Register Windows**

Think of a carousel with several seats. As the carousel spins, each seat passes by the same point. This is similar to how **circle** register windows work.

* **The windows are arranged in a circle**.
* **The window pointer can move in either direction**.
* **This allows for a larger number of windows** without increasing the total number of registers. For example, if you have 10 registers, you can create 10 circular windows, while with sequential windows you might only be able to create 5.

**Sharing Register Windows**

The overlapping region is shared between adjacent windows, enabling efficient data transfer during function calls and returns.

**Q) Explain the Flynn’s classification of computer architectures with diagrams.**

**Flynn's classification** is a way to categorize computer architectures based on how they handle instructions and data. It looks at two main factors:

1. **Instruction streams:** These are the sequences of instructions that the computer executes.
2. **Data streams:** These are the data that the computer processes.

Categories

1. SISD (Single Instruction, Single Data)
2. SIMD (Single Instruction, Multiple Data)
3. MISD (Multiple Instruction, Single Data)
4. MIMD (Multiple Instruction, Multiple Data)

**1. Single Instruction, Single Data (SISD)**

* **Instructions:** Only one instruction is executed at a time.
* **Data:** Only one data item is processed at a time.
* **Example:** A traditional desktop computer with a single processor.

**2. Single Instruction, Multiple Data (SIMD)**

* **Instructions:** Only one instruction is executed at a time, but it operates on multiple data items simultaneously.
* **Data:** Multiple data items are processed in parallel.
* **Example:** A graphics processing unit (GPU) that can perform the same operation on many pixels at once.

**3. Multiple Instruction, Single Data (MISD)**

* **Instructions:** Multiple instructions are executed simultaneously, but they operate on the same data item.
* **Data:** Only one data item is processed at a time.
* **Example:** Not widely used in modern systems

**4. Multiple Instruction, Multiple Data (MIMD)**

* **Instructions:** Multiple instructions are executed simultaneously on multiple data items.
* **Data:** Multiple data items are processed in parallel.
* **Example:** Multiprocessor systems, clusters.

**Q) What are the different types of pipeline hazards? Explain each pipeline hazard with example.**

Pipeline hazards, also known as pipeline conflicts, occur when instructions cannot execute in sequence like one after another because of problems like hardware limitations, needing the result of a previous instruction, or not knowing the next step (like in a branch). These hazards can significantly impact the performance of a processor.

Types of pipeline hazards:

1. Structural Hazards
2. Data Hazards
3. Control Hazards

**Structural Hazards**

* Occur when two or more instructions need the same hardware simultaneously and hardware resources are not available
* **Example:** A processor with a single ALU (Arithmetic Logic Unit) cannot execute two arithmetic operations in the same cycle.

**Data Hazards**

* Occur when an instruction depends on the result of a previous instruction that is still in the pipeline, leading to a stall
* **Example:** Load R1, A

Add R2, R1, B

* The **Add** instruction depends on the result of the **Load** instruction. If the Load is still in the memory access stage, the **Add** will have to stall until the data is available.

**Control Hazards**

* Occur when the pipeline makes decisions based on branch instructions and decide whether to follow one set of instructions or another set of instructions is not known.
* Example:

A computer code with black text

Description automatically generated

When the processor comes across the "**if**" statement, it needs to check the condition to see whether to go to "**label1**" or "**label2**." If it can't decide until later in the process, processor clear out the instructions known as **flushing the pipeline**. The processor has to start fetching and executing the correct instructions from scratch. This slows down the overall execution

**Types of Data Hazards**

Data hazards can be further classified into three types:

* **Read After Write (RAW):** An instruction tries to read a register before a previous instruction writes to it.
* **Write After Read (WAR):** An instruction tries to write to a register before a previous instruction reads from it.
* **Write After Write (WAW):** Two instructions try to write to the same register.

**Mitigation Techniques**

To mitigate pipeline hazards and improve performance, various techniques are employed:

* **Forwarding:** Bypassing the data from one stage to another to avoid stalls.
* **Branch Prediction:** Predicting the outcome of a branch to reduce the impact of control hazards.
* **Delayed Branches:** By inserting a no-operation (nop) instruction after a branch instruction. This delay allows the computer to calculate the correct target address for the branch, reducing the errors.
* **Pipeline Scheduling:** Rearranging instructions to minimize hazards.

Explain the computer components.

**Q) Explain the store-program concept with example.**

The store-program concept is a fundamental concept in computer architecture where both instructions and data are stored in the computer's memory. It allows the computer to fetch, decode, and execute instructions sequentially from memory. This concept was first introduced by John von Neumann.

**How it works:**

1. **Instruction Storage**
2. Program Counter
3. Fetch-Execute Cycle
4. Increment PC

**Instruction Storage**

* Instructions are stored in memory.
* Memory can be volatile (RAM) or non-volatile (ROM).

**Program Counter:** PC holds/track the address of the next instruction to be executed.

**Fetch-Execute Cycle**

1. **Fetch:** PC is used to get the instruction from memory.
2. **Decode:** Understand what the instruction means and what needs to be done.
3. **Execute:** Perform the operation specified by the instruction (like calculations).

**Increment PC:** PC is increased to point to the next instruction.

**Example**

Consider a simple program that adds two numbers, 5 and 3.

1. **Instructions:**

* Load 5 into register A
* Load 3 into register B
* Add the contents of register B to register A
* Store the result in memory location C

1. **Execution:**

* The PC starts at the address of the first instruction.
* The CPU fetches the instruction "Load 5 into register A" and decodes it.
* The CPU loads the value 5 into register A.
* The PC is incremented to the next instruction.
* The process continues for the remaining instructions.

**Q) Define associative memory. Explain with block diagram how it can be implemented**

**Associative memory**, also known as content-addressable memory (CAM), where data is accessed based on its content rather than its address. Instead of looking for data at a specific location, you can search data by providing a key that matches the data. It is often used in applications like cache memory, database searching, where finding data by its content is more practical than searching by its exact location.

Block Diagram Representation

A diagram of a computer program

Description automatically generated

**Explanation of the Block Diagram**

**Argument Register**: This is where the search query (or argument) is entered.

**Key Register:** The key register allows you to specify which parts of the argument to search for.

**Associative Memory Array:** The database containing all stored information.

**Matching Process: The** system compares the argument register's contents with each record in the associative memory, using the filter from the key register. If a record matches, then corresponding bit in the match register will be set to 1.

**Match Register:** Tracks which records (in associative memory) matched the search criteria, with bits set to 1 for matching entries.

**Results:** Displays the matched data after the search is complete.

### Advantages of Associative Memory

1. **Fast Search:** Quickly finds data without scanning the entire memory.
2. **Content-Based Retrieval:** Retrieves data based on its content instead of its memory location.
3. **Database Speedup:** Often used to enhance database performance.
4. **Parallel Processing:** Supports simultaneous searching across multiple entries. This means it can search all relevant data at once instead of checking each record one by one.
5. **Application in Virtual Memory:** Utilized in page tables and neural networks.

### Disadvantages of Associative Memory

1. **Higher Cost:** More expensive than traditional RAM.
2. **Complex Design:** Each cell requires storage and logic circuits for content matching.

### Applications of Associative Memory

1. Database Management Systems: fast data access
2. Image Processing: Used to search for specific patterns within images
3. Artificial Intelligence
4. Networking
5. Memory Allocation

**How does DMA controller work? Give an example of DMA data transfer**

**DMA (Direct Memory Access)** transfer is a method of transferring data between **peripherals** devices and memory without involving the **CPU** in the actual data movement. This allows devices to communicate directly with the system memory, enabling faster data transfers and freeing up CPU resources for other tasks. This is done using a dedicated hardware component called the DMA controller.

A diagram of a computer system

Description automatically generated

**Figure -** DMA Transfer in computer System

DMA system components

1. **DMA Controller:** Manages the entire data transfer process.
2. **System Bus**: collection of wires used to transmit data, addresses, and control signals, which used to communicate with memory and devices.
3. **Main Memory**: Where data is stored or retrieved from.
4. **I/O Device**: The peripheral device involved in the data transfer.

How It Works / Process of DMA Data Transfer

**DMA Request:** The I/O device sends a request to the DMA controller.

**DMA Grant:** The DMA controller grants permission and takes control of the system bus.

**Data Transfer:** The device directly transfers data between its memory and main memory.

**DMA Acknowledge:** The DMA controller signals completion to the device.

**Interrupt:** The DMA controller may send an interrupt to the CPU to notify it of the completed transfer.

**Example of DMA Data Transfer**

**Scenario**: Copying a large file from a USB flash drive to the computer's memory (RAM).

**Process**:

1. **Initiation**: You insert a USB flash drive into your computer and select a large file to copy.
2. **Request**: The operating system (OS) sends a request to the DMA controller to begin the transfer, providing details about the source (USB drive), destination (RAM), and the size of the file.
3. **Grant**: The CPU acknowledges this request and gives permission for the DMA controller to access the system bus.
4. **Transfer**:
   * The DMA controller takes control and instructs the USB controller to send a block of data directly to RAM.
   * Instead of moving data byte by byte, the DMA controller transfers large blocks of data at once, significantly speeding up the process.
5. **Notification**: Once the transfer is complete, the DMA controller sends an interrupt signal to the CPU, notifying it that the operation is finished. The CPU can then check for errors and proceed with other tasks.

**Differentiate between hardwired control unit and a micro programmed control unit.**

|  |  |  |
| --- | --- | --- |
| Feature | Hardwired Control Unit | Microprogrammed Control Unit |
| Definition | Use Logic gates and flip-flops to generate control signals and execute instructions | uses a set of instructions (microinstructions) stored in memory (ROM) to generate control signals and execute instructions |
| Functionality | Fixed, specific tasks | Flexible, can be updated easily |
| Modification Requirements | Difficult to modify | Easier to modify |
| Speed | Faster due to direct hardware operations | Slightly Slower due to fetch decode execute microinstructions |
| Design Complexity | Complex | Simpler |
| Cost | High, since changing functionality requires new hardware | Lower, as updates are done through changes in microinstructions |
| Example Processor | RISC Processors | CISC Processors |

**What is Parallel Processing?**

Parallel processing is a method which used more than one processor to perform different parts of a task at the same time.

It breaks a big job into smaller tasks, with each processor handling a different task simultaneously.

This method speeds up large and complex tasks, by doing multiple calculations at once.

It’s like having a team of workers handling different parts of a big job simultaneously instead of one person doing everything step by step.

A diagram of a process

Description automatically generated

The diagram demonstrates how data from the processor registers can be sent to multiple functional units simultaneously.

**For example:**

* If arithmetic operations are needed, data goes to the Arithmetic Unit
* If logical operations are needed, data goes to the Logic Unit

This allows for parallel execution of different operations.

How Parallel Processing Works

* **Break down the task:** Divide a large task into smaller, manageable parts.
* **Assign tasks:** Assign each part to a different processor or core.
* **Work independently:** Each processor works on its assigned part.
* **Coordinate:** If needed, processors communicate to ensure they're working together correctly.
* **Combine results:** Once all parts are finished, the results are combined to create the final output.

**Types of Parallel processing**

* Single Instruction Multiple Data (SIMD)
* Multiple Instruction Multiple Data (MIMD)
* Multiple Instruction Single Data (MISD)
* Single Program Multiple Data (SPMD)

**Instruction Stream and Data Stream**

* **Instruction stream:** The sequence of instructions read from memory.
* **Data stream:** The operations performed on data in the processor.

**Application of Parallel Processing**

**Weather Forecasting:** Faster, more accurate predictions.

**Graphics:** Real-time visuals and faster animation.

**Data Analysis:** Faster analysis of large datasets.

**Medical Scans (like MRI or CT scans)**

**Financial Modeling:** Faster calculations and simulations.

**Cryptocurrency Mining:** Faster puzzle-solving.

Search Engines (like Google)

Self-Driving Cars and Robots

**Benefits of Parallel Processing**

**Faster tasks:** Work gets done quicker.

**Better efficiency:** Makes the most of your computer's resources.

**Real-time action:** Enables instant responses for things like games and self-driving cars.

**Pipeline**

1. Pipeline Structure
2. Pipeline Processing
3. Register Contents Over Time
4. Space-Time Execution

### Example: Pipeline Processing Diagram


A screenshot of a diagram

Description automatically generated

**Pipeline Structure**

* Think of the pipeline as an assembly line in a factory, where tasks move from one station to the next.
* Data flows **from left to right**, meaning it starts in the first segment and moves to the last segment step by step.

**Register Contents (Table) Over Time**

****

The table has four columns:

1. **Clock Pulse Number:** Tracks the number of clock cycles.
2. **Segment 1:** Shows the task currently being processed in the first stage.
3. **Segment 2:** Shows the task currently being processed in the second stage.
4. **Segment 3:** Shows the task currently being processed in the third stage.

**Pipeline Operation:**

The table illustrates how data moves from one stage to the next.

1. **Initialization:**

* In the first clock cycle (Clock Pulse Number 1), the initial values A1 and B1 are loaded into the registers of Segment 1.

1. **Data Movement and Processing:**

* In the second clock cycle, A1 and B1 move to Segment 2, and new values A2 and B2 are loaded into Segment 1.
* In Segment 2, the operation A1 \* B1 is performed, and the result is stored in a register.
* This pattern continues, with data moving through the pipeline stages and undergoing processing at each stage.

1. **Final Output:**

* The final result of the computation is obtained in the last clock cycle. In this case, it is the value stored in the register of Segment 3.

**Key Points:**

* **Pipeline Stages:** The pipeline has three stages (segments) in this example.
* **Data Flow:** Data moves from one stage to the next in each clock cycle.
* **Parallel Processing:** The pipeline allows for parallel processing of different parts of the task.

**Register Content Table (Six Segment Pipeline with 8 Tasks)**

* **Fetch (F)**: Fetches the instruction.
* **Decode (D)**: Decodes the instruction.
* **Execute (E)**: Executes the instruction.
* **Memory Access (M)**: Reads or writes data.
* **Write Back (WB)**: Writes the result back to the register.
* **Idle (I)**: Indicates no task is being processed in that segment.

**A table with text and numbers

Description automatically generated**

**Explanation:**

* Each row represents a clock cycle.
* Each column represents a pipeline stage.
* The letters T1, T2, ..., T8 represent the eight tasks.
* As the clock cycles progress, tasks move through the pipeline stages, with each stage performing its specific operation.

**What do you mean by pipeline? Explain with space time diagram for a six segmented pipeline showing the time it takes to process eight tasks.**

A pipeline is a technique that works like a step-by-step process, where different parts of data are handled one after the other. Each step takes care of a specific part, allowing several tasks to be worked on simultaneously, but each task is at a different stage in the process.

A diagram of a flowchart

Description automatically generated

**Figure: Six segment pipeline**

* Six processing segments (S₁ to S₆)
* Six registers (R₁ to R₆)
* A single clock signal controlling all registers
* The clock ensures synchronized data movement between segments
* Each register captures data at the clock edge
* Data flows from left to right through the pipeline
* The clock coordinates the movement of data through all stages

A grid of numbers and letters

Description automatically generated

**Figure: space-time diagram for a six-segmented pipeline processing eight tasks**

This diagram illustrates how tasks are processed in a six-segmented pipeline over time. Each row represents a pipeline stage, and each column represents a clock cycle. The letters T1, T2, ... T8 represent the eight tasks being processed.

**How the Pipeline Works:**

1. **Initialization:**

* In the first clock cycle, Task 1 (T1) enters the first stage (S1).

1. **Task Movement:**

* In the second clock cycle, T1 moves to S2, and T2 enters S1.
* In the third clock cycle, T1 moves to S3, T2 moves to S2, and T3 enters S1.

This pattern continues, with each task progressing through the stages.

1. **Completion:**

* Once a task reaches the final stage (S6), it is considered complete. For instance, T1 completes in the seventh clock cycle.

Explain an instruction pipeline with an example.

Pipeline processing is a technique which is used to improve the performance of computer systems by breaking down the execution of instructions into multiple stages allowing different parts of multiple instructions to be processed simultaneously.

**Instruction Cycle**


* 1. Fetch the instruction from memory.
  2. Decode the instruction.
  3. Calculate the memory address.
  4. Fetch the operands(data) from memory/register.
  5. Execute the instruction.
  6. Store the result.

**Four-Segment Pipeline Design**

A diagram of a computer program

Description automatically generated

**Figure:** Four Segment CPU Pipeline



**Figure:** Timing of Instruction Pipeline

**Explanation of Stages:**

* **IF** (Fetch Instruction) - Instruction Fetch - Retrieves the instruction from memory.
* **DA**: **(Decode/Address Calculation)**- Decodes the instruction and calculates any necessary memory addresses.
* **FO**: Fetch Operand - Fetches the operands needed for execution from memory or registers.
* **EX**: Execute - Carries out the instruction (arithmetic, logical operations, etc.).

**Stalls**: The **"-"** in the table represents a stall, indicating that an instruction has to wait for a resource or data to be available. This is common in pipelining, especially when a branch instruction is encountered.

**How is performance of computer increased using pipeline? Explain with practical example?**

Pipeline processing is a technique which is used to improve the performance of computer systems by breaking down the execution of instructions into multiple stages allowing different parts of multiple instructions to be processed simultaneously.

**How Pipelining Increases Performance**

1. Parallel Execution: (Reduces Wait Time)
2. Higher Throughput (Increases the Number of Instructions Processed)
3. Reduced Instruction Latency (Enables Faster Operation)
4. **Improved Clock Rate**
5. Supports Parallelism (Allows for Simultaneous Operations)
6. **Overlapping Execution**

### Pipelining allows different stages of multiple instructions to be processed at the same time, reducing the CPU waiting time

### Higher Throughput

By allowing new instructions to start before previous ones finish, pipelining enables the CPU to complete more instructions in a shorter period time.

1. **Reduced Instruction Latency (Enables Faster Operation)**:

Although the time to execute a single instruction might not change much, pipelining reduces the overall time needed to complete a sequence of instructions.

**Practical Example of Pipelining**

Imagine you’re in a car wash. The car wash has six steps: washing, soaping, scrubbing, rinsing, drying, and polishing. Each of these steps happens in a different section, and the car moves from one section to the next.

**How It Works:**

1. **First Car (Car 1)**: It starts in the first section (washing).
   * While Car 1 is being washed, the other sections are empty.
2. **Second Car (Car 2)**: After Car 1 moves to the next section (soaping), Car 2 enters the first section (washing).
   * Now, two cars are in the car wash, each in a different section.
3. **Third Car (Car 3)**: When Car 1 moves to the third section (scrubbing), Car 2 moves to the second section (soaping), and Car 3 starts in the first section (washing).
4. **Eventually, All Sections Are Busy**: After six cars have entered, every section will be busy with a different car. Now, a new car can enter the car wash every time a car finishes, keeping the whole process moving smoothly.

**What is arithmetic overflow? How can it be detected?**

What is overflow? Explain overflow detection process with signed and unsigned number addition with suitable example

Arithmetic overflow is a situation in which the result of an arithmetic operation (such as addition, subtraction, multiplication, or division) is too large to be represented within the available bits, resulting in an incorrect answer or sign error

**How Can Arithmetic Overflow Be Detected?**

* 1. Sign Bit Analysis
  2. Unsigned Integer Overflow

**Signed Integer Overflow:**

* If two positive numbers are added and the result is negative, overflow has occurred.
* If two negative numbers are added and the result is positive, overflow has occurred.

**Unsigned Integer Overflow:**

* If the carry-out from the most significant bit is 1, overflow has occurred.

**Example of Signed Integer Overflow**

Adding Two Large Positive Numbers

* Add: 127 (Decimal) + 1 (Decimal)

**Binary Representation**:

* 127 in binary (8-bit): **01111111**
* 1 in binary (8-bit): **00000001**

**Addition**

A close-up of a computer screen

Description automatically generated

The expected result of adding 127 and 1 should be **128**, which is not representable in an 8-bit signed integer format (which can only represent from **-128 to +127**).

Since we added two positive numbers (**127 and 1**) but ended up with a negative result **(-128)**, this indicates that **overflow has occurred**.

**Example of Unsigned Integer Overflow**

**Example: Adding Two Unsigned Numbers**

* Add**: 200 (Decimal) + 100 (Decimal)**

**Binary Representation**:

* 200 in binary (8-bit): **11001000**
* 100 in binary (8-bit): **01100100**

**Addition**

A line of circles with red and black circles

Description automatically generated

The result **100001100** exceeds the 8-bit representation. We can only keep the least significant 8 bits, which is **00000100**

There is a carry-out from the most significant bit (the leftmost **1** in **100001100**). Therefore, **overflow has occurred** for unsigned addition.

**Differentiate between instruction pipeline and an arithmetic pipeline.**

|  |  |  |
| --- | --- | --- |
| **Feature** | **Instruction Pipeline** | **Arithmetic Pipeline** |
| Focus | Aims to make the CPU execute instructions faster | Aims to make arithmetic calculations faster |
| Level of Operation | Works at the instruction level | Works at the operation level |
| Stages | Involves stages like fetching, decoding, executing, and writing back | Involves smaller stages for specific operations like addition and multiplication |
| Overlapping | Allows different instructions to be in various stages at the same time | Allows different arithmetic operations to be in various stages at the same time |
| Hazards | Stalls if instructions depend on each other | Stalls if one operation relies on another |
| Goal | Increases the performance of the system | Improve the performance of arithmetic operations |

What is cache memory? Explain the mapping process. Differentiate between direct mapping and associate mapping.

**Mapping => Cache Mapping**

Cache memory is a high-speed memory that acts as a buffer between the CPU and main memory (RAM). It stores copies of frequently accessed data from main memory, allowing the CPU to access it more quickly. Cache memory is typically smaller and faster than main memory, making it a valuable tool for improving system performance.

**Mapping Process in Cache Memory**

The **mapping process** refers to how the addresses from the main memory are translated into cache addresses. Since cache memory is smaller than main memory, so it cannot hold all the data. Mapping determines where data from main memory will be stored in the cache.

A diagram of a computer network

Description automatically generated

Figure: Process of Cache Mapping

**Types of Mapping**

* **Direct Mapping**
* **Associate Mapping**

**Direct Mapping**

1. **Mapping Method:** Each item from the main memory goes to one specific spot in the cache using a modulus operation.
2. **Mapping Formula:** Uses a formula to figure out the spot: **(Block number) mod (Number of cache spots)**.
3. **Example:** If there are 4 spots in the cache and the block number (item) is 6, then **Cache Line = 6 mod 4 = 2**.
4. **Tag Bits:** Needs fewer labels because the spot is always the same.
5. **Access Time:** Quicker because you know exactly where to look.
6. **Conflict Misses:** Higher chance of conflict misses, because different items (blocks) might need the same spot, causing them to replace each other.
7. **Advantages:** Simple implementation, fast access, and less expensive.
8. **Disadvantages:** Multiple items (blocks) may map to the same cache spot, causing replacement of data.

**Associative Mapping**

1. **Mapping Method:** An item can be stored in any available spot in the cache.
2. **Mapping Formula:** No formula is needed; the item can go anywhere there is space.
3. **Example:** If an item is brought into the cache, it can go to any empty spot.
4. **Tag Bits:** Needs more detailed labels since the item (blocks) can be anywhere, and all spots need to be checked.
5. **Access Time:** Slower because you have to check every spot to find the item.
6. **Conflict Misses:** Less likely to happen since items (blocks) can go to any spot, reducing the chance of replacing each other.
7. **Advantages:** Reduced conflict misses.
8. **Disadvantages:** Requires more time to search since the item (blocks) can be anywhere, and all spots need to be checked.

**Direct Mapping vs Associative Mapping**

A screenshot of a computer

Description automatically generated

Describe micro-programmed control unit. Explain different types of addressing modes with example.

or

Explain the various types of addressing modes and compare them algorithm, advantage and disadvantage.

A micro-programmed control unit is a part of the CPU that controls the execution of instructions by generating control signals. It relies on a series of small instructions, called "microinstructions," stored in a special memory known as control memory. These microinstructions produce control signals that directly manage the CPU's hardware components, like registers, the Arithmetic Logic Unit (ALU), and memory.

Key Components of a Micro-Programmed Control Unit:

**Control Memory:** Stores the microprogram, which consists of a sequence of microinstructions.

**Control Address Register (CAR):** Contains the address of the next microinstruction to be executed.

**Microinstruction Register (MIR):** Temporarily holds the current microinstruction being executed.

**Microinstruction Decoder:** Decodes the microinstruction and generates the needed control signals.

A diagram of a basic computer system

Description automatically generated

### How It Works:

When the CPU needs to execute an instruction, the micro-programmed control unit fetches a sequence of microinstructions from control memory. Each microinstruction generates specific control signals to activate parts of the CPU (like registers and the ALU) for each step, allowing even complex instructions to be broken down into simple, controlled operations.

Addressing modes

Addressing modes are different ways of giving instructions to the CPU which finds the location of the data (or operand) it needs for an instruction. Each addressing mode gives specific instructions on where to look for this data, like directly in memory, in a register, or even in the instruction itself.

In short, addressing modes help the CPU understand exactly where to find the information it needs to complete an operation.

common addressing modes:

1. Immediate Addressing:
2. Direct Addressing:
3. Indirect Addressing:
4. Register Addressing:
5. Register Indirect Addressing:

**Immediate Addressing Mode**

* **Definition/Algorithm**: The operand is directly specified within the instruction.
* **Advantage:** Fast, no memory access required.
* **Disadvantage:** Limited operand range, suitable for small constants.
* **Example**: MOV R1, #10  
  This means the value 10 is moved directly to R1. Here, #10 is an immediate operand.

**Direct (Absolute) Addressing Mode**

* **Definition/Algorithm**: The address of the operand is specified directly in the instruction.
* **Advantage:** Simple, efficient for accessing fixed locations.
* **Disadvantage:** Limited address space, requires more memory for the address.
* **Example**: MOV R1, [1000]  
  This moves the value from memory location 1000 to R1.

**Indirect Addressing:**

* **Definition/Algorithm**: The address of the operand is stored in a memory location, and the address of that memory location is specified in the instruction.
* **Advantage:** Flexible, allows for dynamic memory access.
* **Disadvantage:** Slower due to multiple memory accesses
* Example: LOAD R3, (200) (Load the value at the memory location whose address is stored at memory location 200 into register R3)

**Register Addressing:**

* **Definition/Algorithm:** The operand is stored in a register.
* **Advantage:** Very fast, no memory access required.
* **Disadvantage:** can only work with data in registers, not large data
* Example: ADD R4, R5 (Add the contents of register R5 to register R4)

**Register Indirect Addressing:**

* **Definition/Algorithm:** The address of the operand is stored in a register.
* **Advantage:** allows dynamic memory access
* **Disadvantage:** Slower due to multiple memory accesses
* Example: LOAD R6, (R7) (Load the value at the memory location whose address is stored in register R7 into register R6)

**Explain the data transfer and manipulation instruction with example.**

Explain the data transfer instructions with example

Data transfer and manipulation instructions are essential part of assembly language programming. These instructions are used to move data between registers, memory, and I/O devices, as well as to perform operations on that data.

Data Transfer Instructions

Data Manipulation Instructions

Data Transfer Instructions

These instructions are used to move data from one location to another.

**Common Data Transfer Instructions:**

* **LOAD**: This instruction moves data from memory to a register.
* **STORE** This instruction moves data from a register to memory.
* **MOVE**: This instruction moves data between registers.
* **PUSH**: Transfer data onto the stack.
* **POP**: Transfer data from the stack back into a register or memory.

Example:

LD R1, [0x1000]: This instruction **Load** the data from memory address 0x1000 into register R1.

ST R2, [0x2000]: This instruction **Store** the data from register R2 into memory address 0x2000.

MOV R3, R4: This instruction **Copy** the value from Register R3 to Register R4.

Data Manipulation Instructions

These instructions perform operations on data, such as arithmetic, logical, and shift operations.

There are three basic types

1. Arithmetic Instructions:
2. Logical Instructions:
3. Shift Instructions:

Common Data Manipulation Instructions:

**ADD**: Adds two operands

**SUB**: Subtracts one operand from.

**MUL**: Multiplies two operands.

**DIV**: Divides one operand by another.

**AND**, **OR**, **XOR**: Perform bitwise logical operations.

**NOT**: Inverts the bits of an operand.

Example:

ADD R5, R6: This instruction **Add** the values in R5 and R6, store the result in R5

SUB R7, R8: This instruction **Subtract** the value in R8 from R7, store the result in R7

MUL R9, R10: **Multiply** the values in R9 and R10, store the result in R9

DIV R11, R12: **Divide** the value in R11 by R12, store the quotient in R11 and remainder in R12

**Explain common bus system for basic computer.**

A common bus system is a fundamental concept in computer architecture that allows various components to communicate and share data.

A bus is a collection of wires used to transmit data, addresses, and control signals from one system to another.

Types of Buses / Key Components of a Common Bus System

1. **Data Bus:** Carries data to and from memory and I/O devices.
2. **Address Bus:** Specifies the memory location or I/O device address.
3. **Control Bus:** Transmits control signals to coordinate the data transfer.

A diagram of a computer program

Description automatically generated

What do you mean by Register Transfer Language? Explain the use of Register Transfer Language control function.

Register Transfer Language (RTL) is a symbolic language used to describe how data moves between registers and the operations performed on that data in a digital system, like a CPU.

RTL provides a way to describe what happens in each clock cycle—whether it’s moving data from one register to another, performing an arithmetic calculation, or enabling a control signal for a particular part of the system.

Key Concepts in Register Transfer Language:

* **Registers:** Temporary Storage for data and instructions.
* **Data Transfer:** The process of moving data from one register to another and vice versa.
* **Control Signals:** Signals that control the operation (data transfers, arithmetic operations)

### Examples of RTL Expressions:

* R1 <= R2 + R3; – Here, the sum of R2 and R3 is calculated and transferred to R1.
* R1 <= R1 - 1; – This operation decrements the value in R1 by 1 and updates R1 with the result.

### Register Naming Conventions:

Registers are named with capital letters based on their function:

* **Program Counter (PC)**: Tracks the address of the next instruction.
* **Instruction Register (IR)**: Holds the current instruction being executed.

Data Transfer in RTL

**Arrow Notation** : Data transfer uses **Arrow** (<=)

**Connection:** Source register's output must be connected to destination register's input.

**Parallel Loading:** Destination register must support simultaneous loading of multiple bits.

**Timing:** Transfers usually happen on a clock edge for synchronization.

Understanding the RTL Control Functions in Digital Systems

A diagram of a circuit

Description automatically generated

**Block Diagram**:

* **Control Circuit**: This circuit generates the control signal P. When P = 1, it allows data to move from R1 to R2.
* **Load Signal**: The **Control Signal** P activates the **Load Signal** when P=1. Then **Load Signal** tells the destination register R2 to accept data from the source register R1.
* **Clock**: The transfer happens in sync with the clock. When the clock "ticks" (usually going from low to high), data moves from R1 to R2 if P=1.

Timing Diagram:

* **Clock Signal**: Shows the clock cycle going up and down.
* **Load Signal**: Goes high only when P=1. It needs to be high at the right clock tick (at time t) to allow the transfer.
* **Transfer Timing**: The transfer from R1 to R2 happens at time t when the clock edge and the load signal is active.

**Explain the computer components.**

**Computer Components**: The basic parts needed to build a working computer, such as the processor (CPU), memory for storage, and devices for input and output like the keyboard and monitor.

There are 5 main computer components that are given below:

1. Input Unit
2. Output Unit
3. Memory Unit
4. Control Unit
5. Arithmetical and Logical Unit

**A diagram of a computer

Description automatically generated**

**Input and Output Devices (I/O)**

* **Input Devices:** Allow the user to interact with the computer (e.g., keyboard, mouse, scanner).
* **Output Devices:** Parts that show you the computer's results, like a monitor, printer, or speakers.

**Memory Unit**: When you type or enter data into the computer, it’s first stored in the memory unit. Memory unit temporarily holds the information so the computer can work with it. After the computer finishes a task, it also stores the results in the memory unit before showing them to you.

**Control Unit (CU)**

The **Control Unit** acts like the "brain" of the computer. It manages and coordinates everything that happens inside the CPU by interpreting program instructions and sending signals to other components to carry them out.

1. **Memory**: If the processor needs data, the CU tells the memory to send that data. If it has finished using the data, the CU tells the memory to store the results.
2. **Arithmetic/Logic Unit (ALU)**: If the processor needs to perform a calculation (like adding two numbers), the CU tells the ALU to do that specific operation.
3. **Input/Output Devices**: If the processor needs to display something on the screen or send information to a printer, the CU tells those devices what to do.

**Arithmetic Logic Unit (ALU)**: Performs arithmetic and logical operations.

**What do you mean by instruction format? Explain with an example.**

An instruction format is the specific layout of bits in a machine language instruction that tells the computer's processor what operation to perform (ADD, SUB) and where to find the data for operation.

**A close-up of a paper

Description automatically generated**

**Main Parts of an Instruction Format**  
Most instruction formats have two main parts:

1. **Opcode (Operation Code)**: Tells the computer what action to perform, like ADD, SUBTRACT, or LOAD.
2. **Operands/** **Address:** Points to the data location, which might be stored in registers, specific memory locations, or directly within the instruction itself.

Example of an Instruction Format

ADD R1, R2, R3

This instruction tells the processor to add the values in registers R2 and R3 and store the result in R1.

**Opcode**: Specifies the operation (in this case, ADD).

**Destination Operand**: The register where the result will be stored (R1).

**Source Operand(s)**: The registers that hold the values for the operation (R2, R3).

**Binary Representation of Instruction Format**



Here:

* **Opcode**: 00001011 represents the ADD operation.
* **Destination**: 0001 is the code for R1.
* **Source 1**: 0010 is the code for R2.
* **Source 2**: 0011 is the code for R3.

Each field has a fixed number of bits, which the processor decodes to perform the instruction.

Explain the error detection codes with example.

 The binary information is transferred from one location to another location through some communication medium. When data is sent, outside factors (like noise) can cause small changes, flipping parts of the message (changing a 1 to a 0, or vice versa), which leads to errors. To catch these errors, we add a few extra bits, called "redundant bits," to the data. These extra bits help us check if the message we received is the same as the one that was sent, making it easier to spot any mistakes.

The most common error detection codes is

Parity Check

A parity bit is a simple method of error detection that adds a single bit to the end of the data to make the number of 1s either even or odd.

**Types**: There are two types of parity:

* **Even Parity**: The parity bit is set so that the total number of 1s in the data (including the parity bit) is even.
* **Odd Parity**: The parity bit is set so that the total number of 1s is odd.

A diagram of a computer error

Description automatically generated with medium confidence

Explain the non-restoring division algorithm with flow chart, and hardware implementation diagram. Divide 10/3 using restoring division.

Write down the non-restoring division flowchart algorithm and divide 5/3 using non-restoring division.

The non-restoring division algorithm is a method used for performing unsigned binary division. It avoids the restoring step of the restoring division algorithm, which can be time-consuming.

A whiteboard with a diagram and numbers

Description automatically generated

A white board with writing on it

Description automatically generated